A picture containing drawing

Description automatically generated

**LOWERED FLOOR – VW CADDY MAXI**

[](https://tripodmobility.com/wp-content/uploads/2017/08/WAV-Volkswagen-Caddy-Maxi-3.jpg)

* Lowered floor from rear up to 2nd seat row
* 4-point wheelchair tie-down system with an adjustable 3-point seatbelt  for the wheelchair passenger
* Modified fuel tank and exhaust system to accommodate a deep and level lowered floor
* Original seats in the second row are preserved after conversion
* [Ramp](https://tripodmobility.com/en/differences-between-a-clearview-ramp-and-a-taxi-ramp/): Double folding lightweight ramp with clear-view design what allows to view through the back window
* Lowered floor fully covered with matching upholstery
* The center part or the rear bumper will be replaced on hatch, thus maintaining the original look
* The original parking sensors remain functional after conversion

DIMENSIONS

|  |  |
| --- | --- |
| Entrance height: 142 cm/56 inches | Interior height: 147 cm/58 inches |
| Length of lowered floor: 147 cm/58 inches | Width of lowered floor: 81 cm/32 inches |

www.asquithmobilitysolutions.com.au